{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["form(Warranty)","manual(Warranty)"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"form(Warranty)","index":0,"n_rows":116,"n_cols":25,"rows_kept":116,"cut":false,"hidden":false,"merged":[[94,19,95,19],[101,3,101,18],[102,3,102,18],[94,3,94,18],[98,3,98,18],[99,20,99,22],[99,23,99,24],[97,1,97,2],[112,4,112,25],[97,3,97,18],[97,20,97,22],[97,23,97,24],[103,3,103,18],[94,1,95,2],[95,3,95,18],[94,20,95,22],[96,3,96,18],[100,3,100,18],[102,23,102,24],[94,23,95,24],[96,1,96,2],[96,20,96,22],[96,23,96,24],[105,1,105,24],[79,3,79,18],[80,3,80,18],[81,3,81,18],[82,3,82,18],[89,3,89,18],[91,3,91,18],[92,3,92,18],[83,3,83,18],[84,3,84,18],[85,3,85,18],[87,3,87,18],[88,3,88,18],[85,23,87,24],[90,3,90,18],[90,20,90,22],[90,23,90,24],[88,20,88,22],[88,23,88,24],[38,9,38,26],[39,9,39,26],[41,9,41,26],[40,9,40,26],[52,2,56,23],[86,3,86,18],[78,1,78,2],[78,20,78,22],[78,23,78,24],[79,1,81,2],[79,19,81,19],[79,20,81,22],[79,23,81,24],[59,1,59,4],[60,1,60,4],[61,1,63,4],[64,1,64,4],[78,3,78,18],[29,18,29,26],[1,1,1,26],[45,5,45,18],[37,15,37,26],[33,2,33,8],[29,9,29,17],[30,9,30,17],[41,2,41,8],[34,2,34,8],[35,2,35,8],[30,2,30,8],[3,24,3,25],[36,15,36,26],[3,22,3,23],[6,2,6,11],[3,20,3,21],[31,9,31,17],[33,9,33,17],[29,2,29,8],[45,3,45,4],[65,1,65,4],[59,5,59,14],[60,5,60,14],[61,5,63,14],[64,5,64,14],[36,2,37,14],[30,18,35,26],[34,9,34,17],[110,1,110,24],[98,1,98,2],[98,20,98,22],[98,23,98,24],[101,1,101,2],[101,20,101,22],[101,23,101,24],[102,1,102,2],[103,1,103,2],[103,20,103,22],[103,23,103,24],[100,1,100,2],[100,20,100,22],[100,23,100,24],[99,1,99,2],[99,3,99,18],[106,1,106,24],[107,1,107,24],[109,1,109,24],[102,20,102,22],[23,2,23,7],[22,2,22,7],[21,2,21,7],[21,8,21,17],[22,8,22,17],[23,8,23,17],[24,8,24,17],[25,8,25,17],[65,5,65,14],[39,2,39,8],[25,2,25,7],[24,2,24,7],[35,9,35,17],[31,2,31,8],[32,2,32,8],[38,2,38,8],[32,9,32,17],[40,2,40,8],[66,5,66,14],[66,1,66,4],[67,1,67,4],[82,1,84,2],[82,19,84,19],[88,1,88,2],[67,5,67,14],[93,1,93,2],[93,20,93,22],[93,23,93,24],[91,23,91,24],[92,1,92,2],[92,20,92,22],[92,23,92,24],[85,1,87,2],[85,19,87,19],[89,1,89,2],[89,20,89,22],[89,23,89,24],[91,1,91,2],[91,20,91,22],[82,23,84,24],[93,3,93,18],[82,20,84,22],[90,1,90,2],[85,20,87,22]]}
[null,"<Steps for Creation>"]
[null,"(1) See the Manual in the separate sheet and enter the data → (2) Run Check Entry below to confirm → (3) Print Warranty"]
[]
[]
[]
[]
[null,"To"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Warranty of Compliance with PFU’s Requirement for Chemical Substance (Rev.15L01)"]
[]
[]
[null,"We hereby declare and warrant that  we comply with PFU Limited (\"PFU\")'s Group Standard in supplying PFU Group below listed Product, "]
[null,"even if the Product is altered in any elements as far as the Product remains the same in name and part number."]
[]
[]
[null,"We agree that for the purpose of the above warranty, the terms are defined as follows:"]
[]
[]
[null,"1. PRODUCT"]
[]
[null,null,"Survey ID:"]
[null,null,"PFU Group Product Number:"]
[null,null,"Product Name:"]
[null,null,"Manufacturer's P/N  [* Reference]:"]
[null,null,"Manufacturer's Name  [* Reference]:"]
[]
[null,"2. PFU’S GROUP STANDARD"]
[]
[null,null,"RESTRICTED SUBSTANCES",null,null,null,null,null,null,"THRESHOLD",null,null,null,null,null,null,null,null,"REMARK"]
[null,null," (1) Lead and its compounds",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm",null,null,null,null,null,null,null,null,"Make sure to enter exempted applications in the Item 3."]
[null,null," (2) Mercury and its compounds",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (3) Cadmium and its compounds",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 100 ppm"]
[null,null," (4) Hexavalent chromium and Hexavalent\n       chromium compounds",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (5) Polybrominated biphenyls (PBBs)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (6) Polybrominated diphenyl Ethers (PBDEs)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null,"For compliance of  the following  (7) ~ (10) [ PFU Group Standard restriction effective, Jan 22, 2019 ] See Remark at right.　　",null,null,null,null,null,null,null,null,null,null,null,null,"【 Mandatory 】"]
[]
[null,null," (7) Bis(2-ethylhexyl) phthalate (DEHP)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (8) Butyl benzyl phthalate (BBP)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (9) Dibutyl phthalate (DBP)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (10) Diisobutyl phthalate (DIBP)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[]
[null,"3. EXEMPTED APPLICATIONS (See Appendix)"]
[]
[null,null,null,"Exempted Applications"]
[]
[null,null,null,null,null,"↑Select the cell and double click → the Configuration window opens to enter data. No entry is considered to be no exemptions."]
[null,null,null,null,null,"　 * Direct entry is available. See the Configuration Sheet and the note below."]
[null,null,null,null,null,"　　　・Use half-width alphanumeric. Separate applications with a half-width comma (,) if there is more than one."]
[null,"4. REMARKS"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Date (M/D/Y):"]
[null,"Person responsible:"]
[null,"Signature: "]
[]
[]
[null,"Department:"]
[null,"Company:"]
[null,"Phone:"]
[null,"E-mail:"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"[1/2page]"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 2018/10/29 form"]
[]
[null,"Appendix. EXEMPTED APPLICATIONS FROM CONTAINMENT RESTRICTION (REFERENCE LIST)"]
[]
[null,null,"The following table is quoted from the Official Journal of the European Union."]
[null,null,"For any exempted applications other than below, see the Official Journal."]
[]
[null,"No.",null,"EXEMPTED APPLICATIONS FROM CONTAIMENT RESTRICTION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ｐｂ","Ｈｇ",null,null,"Ｃｄ"]
[null,"3(a)",null,"Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,null,null,"for special purposes not exceeding (per lamp):"]
[null,null,null,"　- Short length ( ≤ 500 mm): 3,5 mg may be used per lamp"]
[null,"3(b)",null,"Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,null,null,"for special purposes not exceeding (per lamp):"]
[null,null,null,"　- Medium length ( > 500 mm and ≤ 1500 mm): 5 mg may be used per lamp"]
[null,"3(c)",null,"Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,null,null,"for special purposes not exceeding (per lamp):"]
[null,null,null,"　-  Long length ( > 1,500 mm): 13 mg may be used per lamp"]
[null,"5(b)",null,"Lead in glass of fluorescent tubes not exceeding 0,2 % by weight",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"6(a)-I",null,"Lead as an alloying element in steel for machining purposes containing up to 0,35 % lead by weight \nand in batch hot dip galvanised steel components containing up to 0,2 % lead by weight",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"6(b)-I",null,"Lead as an alloying element in aluminium containing up to 0,4 % lead by weight, \nprovided it stems from lead-bearing aluminium scrap recycling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"6(b)-II",null,"Lead as an alloying element in aluminium for machining purposes with a lead content up to 0,4 % by weight",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"6(c)",null,"Copper alloy containing up to 4 % lead by weight",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"7(a)",null,"Lead in high melting temperature type solders \n(i.e. lead-based alloys containing 85 % by weight or more lead)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"7(c)-I",null,"Electrical and electronic components containing lead in a glass or ceramic other than dielectric ceramic in capacitors, ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,null,null,"e.g. piezoelectronic devices, or in a glass or ceramic matrix compound"]
[null,"7(c)-II",null,"Lead in dielectric ceramic in capacitors for a rated voltage of 125 V AC or 250 V DC or higher",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"8(b)",null,"Cadmium and its compounds in electrical contacts",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"13(a)",null,"Lead in white glasses used for optical applications",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"13(b)-(I)",null,"Lead in ion coloured optical filter glass types",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"13(b)-(II)",null,"Cadmium in striking optical filter glass types; excluding applications falling under point 39 of this Annex\n* Exclusion number 39 (Excluded unused in this regulation): Cadmium included in color conversion II - VI compound semiconductor LED\n   (cadmiumper mm2 of light emitting area <10 μg) for illumination or display system applications.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"13(b)-(III)",null,"Cadmium and Lead in glazes used for reflectance standards",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●",null,null,null,"●"]
[null,15,null,"Lead in solders to complete a viable electrical connection between semiconductor die \nand carrier within integrated circuit flip chip packages",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,34,null,"Lead in cermet-based trimmer potentiometer elements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"form Rev.15L01"]
[null,"* Homogeneous Material"]
[null,"　　\"Homogeneous Material\" means a material that cannot be mechanically disjointed into different materials."]
[null,"　　The term \"Homogeneous\" is understood as \"of uniform composition throughout\", so examples of \"Homogeneous Materials\""]
[null,"　　would be individual types of plastics, ceramics, glass, metals, alloys, paper, board, resins and coatings."]
[null,"　　The term \"mechanically disjointed\" means that the materials can, in principle, be separated by mechanical actions such as"]
[null,"　　unscrewing, cutting, crushing, grinding and abrasive processes."]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"[2/2page]"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 2018/10/29 form"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 2018/10/29 form"]

{"sheet":"manual(Warranty)","index":1,"n_rows":114,"n_cols":25,"rows_kept":114,"cut":false,"hidden":false,"merged":[[101,1,101,2],[101,3,101,18],[101,20,101,22],[101,23,101,24],[102,1,102,2],[102,3,102,18],[102,20,102,22],[102,23,102,24],[98,1,98,2],[98,3,98,18],[98,20,98,22],[98,23,98,24],[99,1,99,2],[99,3,99,18],[99,20,99,22],[99,23,99,24],[100,1,100,2],[100,3,100,18],[100,20,100,22],[100,23,100,24],[95,1,95,2],[95,3,95,18],[95,20,95,22],[95,23,95,24],[96,1,96,2],[96,3,96,18],[96,20,96,22],[96,23,96,24],[97,1,97,2],[97,3,97,18],[97,20,97,22],[97,23,97,24],[91,1,91,2],[91,3,91,18],[91,20,91,22],[91,23,91,24],[92,1,92,2],[92,3,92,18],[92,20,92,22],[92,23,92,24],[93,1,94,2],[93,3,93,18],[93,19,94,19],[93,20,94,22],[93,23,94,24],[94,3,94,18],[88,1,88,2],[88,3,88,18],[88,20,88,22],[88,23,88,24],[89,1,89,2],[89,3,89,18],[89,20,89,22],[89,23,89,24],[90,1,90,2],[90,3,90,18],[90,20,90,22],[90,23,90,24],[29,2,29,8],[29,9,29,17],[29,18,29,26],[30,2,30,8],[30,9,30,17],[30,18,35,26],[31,2,31,8],[31,9,31,17],[3,20,3,21],[3,22,3,23],[3,24,3,25],[6,2,6,11],[24,2,24,7],[24,8,24,17],[25,2,25,7],[35,2,35,8],[35,9,35,17],[25,8,25,17],[21,2,21,7],[21,8,21,17],[22,2,22,7],[22,8,22,17],[23,2,23,7],[23,8,23,17],[36,2,37,14],[36,15,36,26],[37,15,37,26],[38,2,38,8],[38,9,38,26],[32,2,32,8],[32,9,32,17],[33,2,33,8],[33,9,33,17],[34,2,34,8],[34,9,34,17],[45,3,45,4],[45,5,45,18],[51,2,55,23],[58,1,58,4],[58,5,58,14],[59,1,59,4],[59,5,59,14],[39,2,39,8],[39,9,39,26],[40,2,40,8],[40,9,40,26],[41,2,41,8],[41,9,41,26],[65,1,65,4],[65,5,65,14],[66,1,66,4],[66,5,66,14],[77,1,77,2],[77,3,77,18],[60,1,62,4],[60,5,62,14],[63,1,63,4],[63,5,63,14],[64,1,64,4],[64,5,64,14],[77,20,77,22],[77,23,77,24],[78,1,80,2],[78,3,78,18],[78,19,80,19],[78,20,80,22],[78,23,80,24],[79,3,79,18],[80,3,80,18],[111,4,111,25],[104,1,104,24],[105,1,105,24],[106,1,106,24],[108,1,108,24],[81,1,83,2],[81,3,81,18],[81,19,83,19],[81,20,83,22],[81,23,83,24],[82,3,82,18],[83,3,83,18],[84,1,86,2],[109,1,109,24],[84,3,84,18],[84,19,86,19],[84,20,86,22],[84,23,86,24],[85,3,85,18],[86,3,86,18],[87,1,87,2],[87,3,87,18],[87,20,87,22],[87,23,87,24]]}
[null,"<Steps for Creation>"]
[null,"(1) See the Manual in the separate sheet and enter the data → (2) Run Check Entry below to confirm → (3) Print Warranty"]
[]
[]
[]
[]
[null,"To","PFU Limited"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Warranty of Compliance with PFU’s Requirement for Chemical Substance (Rev.15L01)"]
[]
[]
[null,"We hereby declare and warrant that  we comply with PFU Limited (\"PFU\")'s Group Standard in supplying PFU Group below listed Product, "]
[null,"even if the Product is altered in any elements as far as the Product remains the same in name and part number."]
[]
[]
[null,"We agree that for the purpose of the above warranty, the terms are defined as follows:"]
[]
[]
[null,"1. PRODUCT"]
[]
[null,null,"Survey ID:",null,null,null,null,null,-1230001]
[null,null,"PFU Group Product Number:",null,null,null,null,null,"PAXXXX1-XXXX"]
[null,null,"Product Name:",null,null,null,null,null,"Power supply unit"]
[null,null,"Manufacturer's P/N  [* Reference]:",null,null,null,null,null,"ABC-0121XX"]
[null,null,"Manufacturer's Name  [* Reference]:",null,null,null,null,null,"CDE Co."]
[]
[null,"2. PFU’S GROUP STANDARD"]
[]
[null,null,"RESTRICTED SUBSTANCES",null,null,null,null,null,null,"THRESHOLD",null,null,null,null,null,null,null,null,"REMARK"]
[null,null," (1) Lead and its compounds",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm",null,null,null,null,null,null,null,null,"Make sure to enter exempted applications in the Item 3."]
[null,null," (2) Mercury and its compounds",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (3) Cadmium and its compounds",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (4) Hexavalent chromium and Hexavalent\n       chromium compounds",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (5) Polybrominated biphenyls (PBBs)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (6) Polybrominated diphenyl Ethers (PBDEs)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null,"For compliance of  the following  (7) ~ (10) [ PFU Group Standard restriction effective, Jan 22, 2019 ] See Remark at right.　　",null,null,null,null,null,null,null,null,null,null,null,null,"【 Mandatory 】"]
[]
[null,null," (7) Bis(2-ethylhexyl) phthalate (DEHP)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (8) Butyl benzyl phthalate (BBP)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (9) Dibutyl phthalate (DBP)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[null,null," (10) Diisobutyl phthalate (DIBP)",null,null,null,null,null,null," Its concentration in Material(*) shall not exceed 1000 ppm"]
[]
[null,"3. EXEMPTED APPLICATIONS (See Appendix)"]
[]
[null,null,null,"Exempted Applications",null,"7(a),7(c)-I"]
[null,null,null,null,null,"↑Select the cell and double click → the Configuration window opens to enter data. No entry is considered to be no exemptions."]
[null,null,null,null,null,"　 * Direct entry is available. See the Configuration Sheet and the note below."]
[null,null,null,null,null,"　　　・Use half-width alphanumeric. Separate applications with a half-width comma (,) if there is more than one."]
[null,"4. REMARKS"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Date (M/D/Y):",null,null,null,"2018-10-29"]
[null,"Person responsible:",null,null,null,"Taro Fuji, Director"]
[null,"Signature: "]
[]
[]
[null,"Department:",null,null,null,"Quality Assurance Dep."]
[null,"Company:",null,null,null,"ABC Corp.　"]
[null,"Phone:",null,null,null,"xxx-xxx-xxxx"]
[null,"E-mail:",null,null,null,"xxxx@xxxxx.xxxxx.xx.xx"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"[1/2page]"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 2018/10/29 form"]
[]
[null,"Appendix. EXEMPTED APPLICATIONS FROM CONTAINMENT RESTRICTION (REFERENCE LIST)"]
[]
[null,null,"The following table is quoted from the Official Journal of the European Union."]
[null,null,"For any exempted applications other than below, see the Official Journal."]
[]
[null,"No.",null,"EXEMPTED APPLICATIONS FROM CONTAIMENT RESTRICTION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ｐｂ","Ｈｇ",null,null,"Ｃｄ"]
[null,"3(a)",null,"Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,null,null,"for special purposes not exceeding (per lamp):"]
[null,null,null,"　- Short length ( ≤ 500 mm): 3,5 mg may be used per lamp"]
[null,"3(b)",null,"Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,null,null,"for special purposes not exceeding (per lamp):"]
[null,null,null,"　- Medium length ( > 500 mm and ≤ 1500 mm): 5 mg may be used per lamp"]
[null,"3(c)",null,"Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,null,null,"for special purposes not exceeding (per lamp):"]
[null,null,null,"　-  Long length ( > 1,500 mm): 13 mg may be used per lamp"]
[null,"5(b)",null,"Lead in glass of fluorescent tubes not exceeding 0,2 % by weight",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"6(a)-I",null,"Lead as an alloying element in steel for machining purposes containing up to 0,35 % lead by weight \nand in batch hot dip galvanised steel components containing up to 0,2 % lead by weight",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"6(b)-I",null,"Lead as an alloying element in aluminium containing up to 0,4 % lead by weight, \nprovided it stems from lead-bearing aluminium scrap recycling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"6(b)-II",null,"Lead as an alloying element in aluminium for machining purposes with a lead content up to 0,4 % by weight",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"6(c)",null,"Copper alloy containing up to 4 % lead by weight",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"7(a)",null,"Lead in high melting temperature type solders \n(i.e. lead-based alloys containing 85 % by weight or more lead)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"7(c)-I",null,"Electrical and electronic components containing lead in a glass or ceramic other than dielectric ceramic in capacitors, ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,null,null,"e.g. piezoelectronic devices, or in a glass or ceramic matrix compound"]
[null,"7(c)-II",null,"Lead in dielectric ceramic in capacitors for a rated voltage of 125 V AC or 250 V DC or higher",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"8(b)",null,"Cadmium and its compounds in electrical contacts",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"13(a)",null,"Lead in white glasses used for optical applications",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"13(b)-(I)",null,"Lead in ion coloured optical filter glass types",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"13(b)-(II)",null,"Cadmium in striking optical filter glass types; excluding applications falling under point 39 of this Annex\n* Exclusion number 39 (Excluded unused in this regulation): Cadmium included in color conversion II - VI compound semiconductor LED\n   (cadmiumper mm2 of light emitting area <10 μg) for illumination or display system applications.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,"13(b)-(III)",null,"Cadmium and Lead in glazes used for reflectance standards",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●",null,null,null,"●"]
[null,15,null,"Lead in solders to complete a viable electrical connection between semiconductor die \nand carrier within integrated circuit flip chip packages",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,34,null,"Lead in cermet-based trimmer potentiometer elements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"●"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"form Rev.15L01"]
[null,"* Homogeneous Material"]
[null,"　　\"Homogeneous Material\" means a material that cannot be mechanically disjointed into different materials."]
[null,"　　The term \"Homogeneous\" is understood as \"of uniform composition throughout\", so examples of \"Homogeneous Materials\""]
[null,"　　would be individual types of plastics, ceramics, glass, metals, alloys, paper, board, resins and coatings."]
[null,"　　The term \"mechanically disjointed\" means that the materials can, in principle, be separated by mechanical actions such as"]
[null,"　　unscrewing, cutting, crushing, grinding and abrasive processes."]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"[2/2page]"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," 2018/10/29 form"]